Report

Assembler

Read file and find .text part.

How to handle comments

How to handle different type label, different line or same line.

After finishing reading one instruction, get a vector containing typical information. For example, …

Finally, the instructions put into a vector in order.

Next, translate instructions into machine code.

Recognize the instruction type, add or addi or adds …

How to translate machine code of label.